Open topic with navigation

# Example Configurations

This section includes example configurations that demonstrate how to chain two HPE Media Servers.

The following configuration, for the upstream HPE Media Server, runs face detection and then sends the records to a HPE Media Server at `gpu-mediaserver:14000`:

    [Ingest]
    IngestEngine=AV

    [AV]
    Type=LibAV

    [Analysis]
    AnalysisEngine=FaceDetect

    [FaceDetect]
    Type=FaceDetect
    FaceDirection=Front
    MinSize=200
    SizeUnit=pixel

    [Output]
    OutputEngine0=FurtherProcessing

    [FurtherProcessing]
    Type=Post
    Input=FaceDetect.ResultWithSource
    Host=gpu-mediaserver
    Port=14000
    ConfigName=DownstreamFaceRec

The following configuration, for the downstream HPE Media Server, runs face recognition on records received from other Media Servers. To match the upstream configuration, above, this should be saved as `DownstreamFaceRec.cfg`, in the folder specified by the `ConfigDirectory` parameter on the downstream HPE Media Server.

    [Ingest]
    IngestEngine=RecordsFromUpstream

    [RecordsFromUpstream]
    Type=Receive
    Input=FaceDetect.ResultWithSource

    [Analysis]
    AnalysisEngine0=FaceRecognition

    [FaceRecognition]
    Type=FaceRecognize
    Input=RecordsFromUpstream.FaceDetect.ResultWithSource
    RecognitionThreshold=60
    MaxRecognitionResults=1

    [Output]
    OutputEngine0=IDOL

    [IDOL]
    Type=IDOL
    Input=FaceRecognition.Result
    IdolHost=content
    IdolPort=9000
    IdolDB=BroadcastVideo
    Mode=Time
    OutputInterval=60
    XslTemplate=./xsl/toIDX.xsl

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm