Open topic with navigation

# QueueTimeout

The maximum amount of time that a request from an upstream HPE Media Server can remain in the queue. If this timeout is exceeded then the request is removed from the queue and an error is returned to the upstream HPE Media Server.

Type: | Time duration The value of this parameter is a time duration. Specify the duration in the following format:
         1days 2hours 3minutes 4seconds 500milliseconds 600microseconds
You can omit any of the individual durations when they are not required:
         4seconds 500milliseconds
You can also shorten the string by abbreviating the units to their first letter (milliseconds abbreviates to ms, microseconds to us):
         4s 500ms
The following are all equivalent:
         1minute 3seconds
         1m 3s
         63s
Default: | 60s
Required: | No
Configuration Section: | Chaining
Example: | `QueueTimeout=10s`
See Also: | MaxSessions

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm