Open topic with navigation

# AudioChannels

The number of channels that HPE Media Server should request from your License Server for audio analysis.

For more information about allocating channels, see Channels Configuration Parameters.

This parameter affects the maximum number of `process` actions (that include audio analysis) that can run simultaneously. For example, if you set `AudioChannels=3`, HPE Media Server can run up to three `process` actions that include audio analysis at the same time. If a `process` action requests audio analysis and a channel is not available, the `process` action will fail. To ensure that `process` actions do not fail as a result of insufficient audio channels being available, set this parameter to the number of `process` actions that your HPE Media Server is configured to run simultaneously.

Type: | Integer
Default: | 0
Required: | Required to analyze audio
Configuration Section: | Channels
Example: | `AudioChannels=1`
See Also: | SurveillanceChannels VideoManagementChannels VisualChannels

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm