Open topic with navigation

# Ingest MxPEG Video from a File or Stream

HPE Media Server can ingest MxPEG video (but not the audio) from a file or stream.

To ingest MxPEG video

1. Create a new configuration to send to HPE Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Ingest]` section, set the following configuration parameters:

   `IngestEngine` | The name of a section in the configuration file that will contain the ingestion settings.
   `IngestRate` | To ingest MxPEG video from a stream, set this parameter to `1`. To ingest MxPEG video from a file set this parameter to `0`. `IngestRate=1` is not supported with MxPEG files.

   For example:

       [Ingest]
       IngestEngine=MXPEG_STREAM
       IngestRate=1

3. Create a new section in the configuration file to contain the ingestion settings, and set the following parameters:

   `Type` | The ingest engine to use. Set this parameter to `MxPEG`.

   For example:

       [MXPEG_STREAM]
       Type=MxPEG

   TIP:

   There is no configuration parameter to specify the source. You must specify the path of the file or the URL of the stream that you want to ingest as the value of the `Source` parameter in the `Process` action, when you start processing.

   For more information about the parameters you can set to configure ingestion, refer to the HPE Media Server Reference.

4. Save and close the configuration file. HPE recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm