Open topic with navigation

# Location

A comma-separated list of ISO-3166 codes to specify the locations for which you want to recognize number plates. Specify the locations in descending priority. For example, if you are recognizing number plates in France but also want to recognize plates from Germany and Belgium, set this parameter to `Location=FR,DE,BE`.

There are significant differences in the number plates used by countries and states, so setting this parameter is necessary to read the plates successfully.

To obtain a list of supported locations with ISO-3166 codes, use the action ListNumberPlateLocations.

If you want to read plates for a location that is not supported, you can set `Location=NOF` (to recognize plates without matching detected characters to number plate formats).

Type: | String
Default: |
Required: | Yes
Configuration Section: | TaskName
Example: | `Location=US-ME`
See Also: |

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm