Open topic with navigation

# ServiceStatusClients

The IP addresses or names of clients that can request status information from a service. Separate multiple individual addresses with commas. There must be no space before or after the comma.

Adding a client to `ServiceStatusClients` does not enable it to send service control actions. To enable a client to send service control actions, you must add the IP address or host name to the ServiceControlClients.

You can use wildcards in the IP addresses. For example, type `187.*.*.*` to permit any machine whose IP address begins with `187` to access the service's status. You can also filter the `ServiceStatusClients` parameter using CIDR notation.

You can also configure client permissions by using the `[AuthorizationRoles]` configuration section. This section provides a more flexible method for setting up user authorization, and also allows you to set up permissions by using SSL identities or GSS principals. See Authorization Roles Configuration Parameters.

To disable authorization by client IP address, set this parameter to `""`. In this case, HPE Media Server uses the options that you set in the `[AuthorizationRoles]` section only.

Type: | String
Default: | None
Required: | Yes
Configuration Section: | Service
Example: | `ServiceStatusClients=localhost,127.0.0.1`
See Also: | ServiceACIMode ServiceControlClients ServiceHost ServicePort

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm