Open topic with navigation

# Post Output Engine

The `Post` output engine sends records to another HPE Media Server for further processing.

Configuration Parameter | Description
--- | ---
ConfigName | The name of the configuration file that the downstream HPE Media Server must use to process the records that are sent.
Host | The host name or IP address of the HPE Media Server to send the records to.
Input | A comma-separated list of the tracks that you want to send.
Port | The ACI port of the HPE Media Server to send the records to.
Type | The type of output engine to use. Set this parameter to `Post`.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm