Open topic with navigation

# Identify Speakers

NOTE:

Before IDOL Speech Server can identify speakers, you must train the Speech Server. Without training, Speech Server can divide the audio into different speakers and identify the gender of each speaker. For information about training IDOL Speech Server, refer to the IDOL Speech Server Administration Guide.

To identify speakers in video

1. Create a new configuration to send to HPE Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Analysis]` section, add a new analysis task by setting the `AnalysisEngineN` parameter. You can give the task any name, for example:

       [Analysis]
       AnalysisEngine0=IDspeakers

3. Create a new section to contain the settings for the task, and set the following parameters:

   `Type` | The analysis engine to use. Set this parameter to `speakerid`.
   `Input` | (Optional) The audio track to process. If you do not specify an input track, HPE Media Server processes the first track of the correct type produced by the ingest engine.
   `SpeakerIDServers` | The host name and ACI port of an IDOL Speech Server. Separate the host name and port with a colon (for example, `speechserver:13000`). You can specify multiple IDOL Speech Servers by using a comma-separated list. HPE Media Server can connect to only one IDOL Speech Server at a time, but you can provide multiple servers for failover. TIP: You can specify a default IDOL Speech Server to use for all speaker identification tasks by setting the `SpeakerIdServers` parameter in the `[Resources]` section of the HPE Media Server configuration file.
   `TemplateSet` | (Optional) The path to the audio template set file (`.ivs` file) to use for speaker identification. You must create this file. Specify the path relative to the directory defined by the `SpeakerIDDir` parameter in the IDOL Speech Server configuration file. If you do not set this parameter Speech Server cannot identify speakers, but can divide the audio into different speakers and detect the gender of each speaker.
   `SampleFrequency` | (Optional) The sample frequency of the audio to send to the IDOL Speech Server for analysis, in samples per second (Hz). IDOL Speech Server accepts audio at either 8000Hz or 16000Hz.

   For example:

       [IDspeakers]
       Type=speakerid
       SpeakerIDServers=speechserver:13000
       TemplateSet=speakers.ats

   For more information about the parameters that you can use to configure this task, refer to the HPE Media Server Reference.

4. Save and close the configuration file. HPE recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm