Open topic with navigation

# Example Configuration

The following is an example configuration that demonstrates how to detect text in ingested images. The configuration includes a transformation task to draw the region(s) and an encoding task to output the resulting image(s).

    [Ingest]
    IngestEngine=Image

    [Image]
    Type=Image

    [Analysis]
    AnalysisEngine0=DetectText

    [DetectText]
    Type=TextDetection
    DetectionThreshold=50

    [Output]
    OutputEngine0=Response

    [Response]
    Type=Response
    Input=DetectText.Result

    [Transform]
    TransformEngine0=Draw

    [Draw]
    Type=Draw
    Input=DetectText.ResultWithSource
    Color=Red
    Thickness=3

    [Encoding]
    EncodingEngine0=EncodeImage

    [EncodeImage]
    Type=ImageEncoder
    ImageInput=Draw.Output
    OutputPath=output/%session.token%/%segment.sequence%-%source.filename%

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm