Open topic with navigation

# Install HPE Query Manipulation Server on Windows

Use the following procedure to install HPE Query Manipulation Server on Microsoft Windows operating systems, by using the IDOL Server installer.

The IDOL Server installer provides the major IDOL components. It also includes License Server, which HPE Query Manipulation Server requires to run.

To install HPE Query Manipulation Server

1. Double-click the appropriate installer package:

       IDOLServer_VersionNumber_Platform.exe

   where:

   `VersionNumber` | is the product version.
   `Platform` | is your software platform.

   The Setup dialog box opens.

2. Click Next.

   The License Agreement dialog box opens.

3. Read the license agreement. Select I accept the agreement, and then click Next.

   The Installation Directory dialog box opens.

4. Specify the directory to install HPE Query Manipulation Server (and optionally other components such as License Server) in. By default, the system installs on `C:\HewlettPackardEnterprise\IDOLServer-VersionNumber`. Click to choose another location. Click Next.

   The Installation Mode dialog box opens.

5. Select Custom, and then click Next.

   The License Server dialog box opens. Choose whether you have an existing License Server.

   - To use an existing License Server, click Yes, and then click Next. Specify the host and ACI port of your License Server, and then click Next.
   - To install a new instance of License Server, click No, and then click Next. Specify the ports that you want License Server to listen on, and then type the path or click and navigate to the location of your HPE license key file (`licensekey.dat`), which you obtained when you purchased HPE Query Manipulation Server. Click Next.

   The Component Selection dialog box opens.

6. Click Next.

7. Select the check boxes for the components that you want to install, and specify the port information for each component, or leave the fields blank to accept the default port settings.

   For the HPE QMS, you can specify the following ports:

   ACI Port | The port that client machines use to send ACI actions to the HPE QMS. Default: 16000
   Service Port | The port that client machines use to send service requests to the HPE QMS. Default: 16002

   If you do not specify a value, the installer uses the specified default ports.

   Click Next or Back to move between components.

8. After you have specified your settings, the Summary dialog box opens. Verify the settings you made and click Next.

   The Ready to Install dialog box opens.

9. Click Next.

   The Installing dialog box opens, indicating the progress of the installation. If you want to end the installation process, click Cancel.

10. After installation is complete, click Finish to close the installation wizard.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm