Open topic with navigation

# Port

The `Port` parameter specifies the port that is used to send ACI actions to the ACI server.

Type: | Long
Default: |
Required: | No
Allowed Range: | Minimum: 1 Maximum: 65535
Recommended Range: | Minimum: 1025 Maximum: 65535
Configuration Section: | Server
Example: | `Port=7008`
See Also: | AdminClients ProxyClients QueryClients

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm