Open topic with navigation

# IDOLServer`N` Configuration

In the `[DistributionIDOLServers]` section you must create a `[IDOLServer` `N``]` subsection for each IDOL server that the Distributed Action Handler communicates with. Each `[IDOLServerN]` subsection specifies the host and ACI port of a child IDOL server. See Child Server Configuration Parameters.

NOTE:

You must number child IDOL server sections in consecutive order, starting from 0 (zero).

For example:

    [DistributionIDOLServers]
    Number=2

    [IDOLServer0]
    Host=localhost
    Port=9000

    [IDOLServer1]
    Host=1.23.45.6
    Port=9000

ACIEncryption

DefaultRelevance

GSSServiceName

Host

HostPortAlias

Krb5Realm

Krb5Service

MirrorName

MSWindows

Name

Port

Priority

QueryFormat

QueryURI

RequiresAuthentication

ResponseFormat

SecurityKeys

SecurityType

SSLConfig

Type

Weight

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm