Open topic with navigation

# Port

The `Port` parameter specifies the port that is used to send ACI actions to the ACI server.

You must configure Authorization Roles Configuration Parameters to determine the users that can send actions to the server.

Type: | Long
Default: |
Required: | No
Allowed Range: | Minimum: 1 Maximum: 65535
Configuration Section: | Server
Example: | `Port=7008`
See Also: | Authorization Roles Configuration Parameters ProxyClients

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm