Open topic with navigation

# ACI Encryption Configuration Parameters

You can encrypt communications between ACI servers (for example, License Server and License Server) and any applications that use the ACI API by configuring an `[ACIEncryption]` section in each of the application configuration files.

NOTE:

Instead of using ACI encryption, HPE recommends configuring Secure Socket Layer (SSL) connections between ACI servers and applications. For more information, see Secure Socket Layer Parameters.

You can use GSS authorization without using ACI encryption by configuring the GSSServiceName and RequireGSSAuth parameters.

For example:

    [ACIEncryption]
    CommsEncryptionType=GSS
    ServiceName=Kerberos

CommsAllowUnencrypted

CommsEncryptionType

ServiceName

## See Also

Secure Socket Layer Parameters.

© 2017 Hewlett Packard Enterprise Development LP | Send documentation feedback to HPE Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to AutonomyTPFeedback@hpe.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_HP_HTML5_bannerTitle.htm