Open topic with navigation

# PingPeriodInSec

The ping period (in seconds) on child servers that are currently marked `UP`. (TimeBetweenRetries determines the ping interval of child servers that are currently marked `DOWN`.)

`UP` servers do not need as frequent monitoring as `DOWN` servers because their status is confirmed by the fact that they are serving requests.

A `DOWN` server cannot be marked `UP` except by pinging. An `UP` server can be marked `DOWN` if it fails to respond to any query. The status of an `UP` server is updated whenever it responds (or fails to respond) to a query or a ping. Distributed Action Handler only pings an `UP` server if a period of time longer than the value specified by `PingPeriodInSec` has elapsed since the last update of the server status.

Type: | Long
Default: | 60
Allowed Range: | Minimum: 1 Maximum: 32000000
Recommended Range: | Minimum: 60 Maximum: 86400
Required: | No
Configuration Section: | Server
Example: | `PingPeriodInSec=60`
See Also: | PingTimeout TimeBetweenRetries

© 2018 EntIT Software LLC, a Micro Focus company | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm