Open topic with navigation

# Milestone Output Engine Configuration Parameters

The Milestone output engine sends information from Media Server to Milestone XProtect Enterprise or Milestone XProtect Corporate. Each record registers as an event with the Milestone surveillance system.

NOTE:

You must set up your Milestone system to accept data from Media Server.

This section describes the parameters that you can set in the configuration section for a Milestone output task.

Configuration Parameter | Description
--- | ---
GUID | The Milestone GUID of the camera that the events should be associated with.
Host | The host name or IP address of the Milestone XProtect system.
Input | A comma-separated list of the tracks that you want to output.
Location | Location metadata to send with the event.
Port | The Milestone XProtect server port.
ProxyTrack | The `Proxy` track generated by the Milestone ingest engine.
SavePostXML | Specifies whether to save the data produced by the engine (after XSL transformation).
SavePreXML | Specifies whether to save records received by the engine.
Type | The type of output engine to use. Set this parameter to `MilestoneOutput`.
XMLOutputPath | The directory in which to write pre- and post- XML files.
XSLTemplate | The XSL template to use to transform records into events that can be sent to Milestone XProtect.

© 2018 EntIT Software LLC, a Micro Focus company | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm