Open topic with navigation

# Gb_MinDuration

The `GB_MinDuration` parameter specifies the minimum time duration for a sequence of tones, in breaking glass detection.

Type: | Integer
Default: | 50
Recommended Range: | 25–100
Required: | No
Configuration Section: | audiosec module
Example: | `Gb_MinDuration=50`
See Also: |

© 2015-2018 EntIT Software LLC, a Micro Focus company | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm