Open topic with navigation

# Gb_EdgeTrigger

The `Gb_EdgeTrigger` parameter specifies the glass break edge trigger threshold for detecting the initial impact.

Type: | Decimal
Default: | 2.0
Range: | 1.0–32.0 0.0 disables the parameter.
Required: | No
Configuration Section: | audiosec module
Example: | `Gb_EdgeTrigger=2.0`

© 2015-2018 EntIT Software LLC, a Micro Focus company | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm