Open topic with navigation

# Receive Ingest Engine

The Receive ingest engine ingests information (images or video frames, and metadata) that was output by another Media Server. For information about how to split processing across multiple Media Servers, refer to the Media Server Administration Guide.

To configure a task that uses the Receive ingest engine, you can set the following parameters:

Configuration Parameter | Description
--- | ---
Input | A comma-separated list of tracks to receive from the other Media Server.
Type | The type of ingest engine to use. Set this parameter to `Receive`.

The engine produces a track for each track specified by the `Input` parameter. For example, if you set `Input=FaceDetect.ResultWithSource`, the engine produces a track named `taskName.FaceDetect.ResultWithSource`, where `taskName` is the name of the Receive ingest task.

© 2018 Micro Focus or one of its affiliates | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm