Open topic with navigation

# CameraLogicalID

The logical ID of the camera to associate events with. The logical ID is assigned by Genetec Security Center. For information about finding the logical ID, refer to the Genetec Security Center documentation.

If you are ingesting video using the Genetec ingest engine, you do not need to set this parameter. Media Server obtains the logical ID for the camera providing the video.

Type: | String
Default: |
Required: | Required only if you do not ingest video through the Genetec ingest engine
Configuration Section: | TaskName
Example: | `CameraLogicalID=1`
See Also: |

© 2018 Micro Focus or one of its affiliates | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm