Open topic with navigation

# MulticastInput

The `MulticastInput` action specifies whether video from a camera is distributed over multicast.

Parameter | Description
--- | ---
`input` | An integer that specifies the video input (camera).
`enable` | A Boolean that specifies whether video is distributed.
`address` | These parameters are optional. You can use these parameters to change the multicast address. `Address` specifies the IP address and `baseport` specifies the port. The address should be a valid multicast address in the range `224.*.*.*` to `239.*.*.*` The default multicast address is `227.0.0.1` on port `56000`+ (inputnumber `*` 4). For example, the 8th camera (input 7) will multicast on `227.0.0.1:56028`.
`baseport`

## Example

`http://localhost:15000/action=MulticastInput&input=0&enable=true`

© 2018 Micro Focus or one of its affiliates | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm