Open topic with navigation

# Stream Recorded Video

To stream recorded video from VMS, use the following URL:

    rtsp://host:port/Accs=Fifo/strack=storage/utc_start=start-utc_end=end/

where:

`host` | is the host name or IP address of the machine hosting VMS.
`port` | is the RTSP port, as defined by the Port parameter in the `[RTSP]` section of the configuration file. You can also find the RTSP port by using the action GetRtspPort.
`storage` | is the index number of the storage area that contains the video to stream.
`start` | is the start time, as a number of epoch seconds, followed by a period (`.`), followed by the frame number.
`end` | is the end time, as a number of epoch seconds, followed by a period (`.`), followed by the frame number. The value `-1` specifies no end, so that video is streamed indefinitely (unless the recording ends).

For example, to stream recorded video from the fourth storage area, starting from the first frame recorded on 14 February 2018 at 12:13:20, use the following URL:

    rtsp://vms:554/Accs=Fifo/strack=3/utc_start=1518610400.1-utc_end=-1/

© 2018 Micro Focus or one of its affiliates | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm