Open topic with navigation

# LegacyPort

The number of a port to listen on for ACI actions, in addition to the port specified by Port.

Set this parameter if you are replacing your VIS and Wittwin components with VMS, and you need to accept requests from applications that expect to communicate with VIS and Wittwin on different ports.

Type: | Integer
Default: | VMS listens only on the port specified by Port
Required: | No
Configuration Section: | Server
Example: | `LegacyPort=8515`

© 2018 Micro Focus or one of its affiliates | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm