Open topic with navigation

# Port

The port to use to accept RTSP requests. (VMS can stream video to other components). The ports used for streaming are specified by the parameters RtpBasePort and RtpMaxPorts.

Type: | Integer
Default: | 554
Required: | No
Configuration Section: | RTSP
Example: | `Port=554`
See Also: | RtpBasePort RtpMaxPorts

© 2018 Micro Focus or one of its affiliates | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm