Open topic with navigation

# RtpBasePort

The first port used for streaming video in response to an RTSP request.

VMS uses a range of ports, starting from the `RtpBasePort` and stopping at `RtpBasePort` + RtpMaxPorts.

Type: | Integer
Default: | 56000
Required: | No
Configuration Section: | RTSP
Example: | `RtpBasePort=56000`
See Also: | RtpMaxPorts

© 2018 Micro Focus or one of its affiliates | Send documentation feedback to Micro Focus Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm