# SSLConfig

Identifies the configuration section in which the SSL configuration details for distributed engines are specified, usually `SSLOptionN`. You must set this parameter if you are using SSL connections between DAH and child engines.

Setting this parameter in the `[Server]` section controls incoming ACI calls.

Setting this parameter in the `[DistributedEngineN]` section controls outgoing ACI calls to child engines in a Standalone DAH system.

Setting this parameter in the `[IDOLServerN]` section controls outgoing ACI calls to child engines in a DAH system Integrated with IDOL.

Setting this parameter in the `[DAHEngineN]` section controls outgoing ACI calls to child engines in a DAH system Integrated with IDOL in which DAH and DIH child engines are configured separately.

NOTE: You can set this parameter in the `[Server]` section alone, in `[DistributedEngineN]`, `[DAHEngineN]`, or `[IDOLServerN]` alone, or in both the `[Server]` and either `[DistributedEngineN]`, `[DAHEngine]`, or `[IDOLServerN]` sections, depending on how you want to manage your connections.

Type: | String
Default: |
Required: | No
Configuration Section: | Server
Example: | `[DistributedEngine0] SSLConfig=SSLOption0` In this example, the SSL connection to `DistributedEngine0` is configured in the `SSLOption0` section. `[Server] SSLConfig=SSLOption [DistributionIDOLServers] Number=2 [IDOLServer0] SSLConfig=SSLOption [IDOLServer1] SSLConfig=SSLOption1` In this example, incoming ACI calls and outgoing calls to `IDOLServer0` use the same SSL configuration, but outgoing calls to `IDOLServer1` use a different SSL configuration.
See Also: | Secure Socket Layer Parameters

_FT_HTML5_bannerTitle.htm