Media Server 12.11

# Image Classification

Image classification classifies images. The input images could be entire images or video frames, or regions of images or video frames. Classification chooses between the classes that you have created within a classifier.

Before using image classification, you must train a classifier. For instructions that describe how to train Media Server, refer to the Media Server Administration Guide.

Configuration Parameter | Description
--- | ---
ClassificationThreshold | The minimum confidence score necessary for Media Server to output a classification result.
Classifier | The classifier to use for classification.
GPUBatchingDuration | The maximum amount of time to wait, before sending a batch of video frames to the GPU for analysis.
GPUNumParallel | The maximum number of video frames to analyze concurrently using the GPU (per CPU thread).
Input | The name of the track to analyze.
MaxClassResults | The maximum number of classifications to produce for each input record or event.
MaxInputQueueLength | Can be used to place a limit on latency.
NumParallel | The maximum number of CPU threads to use for analysis.
Region | A region of the frame to restrict processing to.
RegionUnit | (Deprecated) The units that the Region parameter uses to specify the size and position of a region.
RestrictToInputRegion | (Deprecated) Specifies whether to analyze a region of the input image or video frame that is specified in the input record, instead of the entire image.
SampleInterval | The interval at which frames are selected to be analyzed.
SegmentDuration | The maximum duration of a record in the `SegmentedResult` or `SegmentedResultWithSource` track.
SyncDatabase | Specifies whether to synchronize with the training database before beginning the analysis task.
Type | The analysis engine to use. Set this parameter to `ImageClassification`.
VariableState | Specifies whether there are multiple classes in the image classifier that represent different states of the same type of object.

## Output Tracks

Output track | Description | Output1 This column indicates whether the information contained in the track is included by default in the output created by an output task (when you don't set the Input parameter for the output task).
--- | --- | ---
`Data` | Contains one or more records, describing the analysis results, for each input record. To limit the number of classifications for each input record, set the MaxClassResults parameter. | No
`DataWithSource` | The same as the `Data` track, but each record also includes the source frame. | No
`Result` | Contains one or more records, describing the analysis results, for each event. When the input is images, Media Server classifies each image separately. When the input is video from an ingest engine, or an engine that does not support tracking, Media Server begins a new result when the classification changes significantly. When the input is video from an engine that supports tracking (for example number plate recognition), results begin and end at the times provided by the other analysis task (for example when the vehicle appears and disappears). The IDs used for the image classification records are also inherited from the input records. To limit the number of classifications for each event, set the MaxClassResults parameter. | Yes
`ResultWithSource` | The same as the `Result` track, but each record also includes the best source frame. | No
`SegmentedResult` | (Available only when processing video). The same as the `Result` track, except the duration of each record is limited by the parameter SegmentDuration. If a result exceeds the specified duration, Media Server begins a new record with the same ID. | Yes
`SegmentedResultWithSource` | (Available only when processing video). The same as the `ResultWithSource` track, except the duration of each record is limited by the parameter SegmentDuration. If a result exceeds the specified duration, Media Server begins a new record with the same ID. | No
`Start` | The same as the `Data` track, except it contains only the first record of each event. | No
`End` | The same as the `Data` track, except it contains only the last record of each event. | No

© Copyright 2022 Micro Focus or one of its affiliates
Version 12.11 | Last updated February 2022

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to swpdl.idoldocsfeedback@microfocus.com.

We appreciate your feedback!

Product: IDOL Media Server 12.11

Topic Title: Image Classification