Media Server 12.11

# Barcode Analysis Results

The following XML is a single record produced during barcode analysis:

    <record>
      ...
      <trackname>barcode.Result</trackname>
      <BarcodeResult>
        <id>b8c4331e-6058-4786-83d9-a43e605f463e</id>
        <text>some text</text>
        <barcodeType>Code-128</barcodeType>
        <region>
          <left>94</left>
          <top>66</top>
          <width>311</width>
          <height>98</height>
        </region>
        <parentID>4d69390f-a8c4-4c5d-a0b0-705a3f98aa9b</parentID>
      </BarcodeResult>
    </record>

The record includes the following information:

- The `id` element provides a unique identifier for the detected barcode. The barcode analysis engine issues an ID for each detected appearance of a barcode. If you are detecting barcodes in video and consecutive frames show the same barcode in a near-identical location, all records related to that appearance will have the same ID.

  For example, if a barcode appears in the same location for fifty consecutive video frames, the engine uses the same ID for each record in the data track and produces a single record in the result track. The record in the result track will have a timestamp that covers all fifty frames.

  If the barcode moves to a different location on the screen, or disappears and then reappears, the engine considers this as a new detection and produces a new ID and a new record in the result track.

- The `text` element contains the data encoded by the barcode. If Media Server detects a barcode with a supplement, for example EAN-13+EAN-2, the `text` element contains the digits from both parts of the barcode, separated by a hyphen.

- The `barcodeType` element contains a string which describes the type of the detected barcode. This can be any of the following values:

  Codabar Code-128 Code-39 Code-93 Datalogic 2/5 Data Matrix EAN-13 EAN-13+EAN-2 EAN-13+EAN-5 EAN-8 EAN-8+EAN-2 EAN-8+EAN-5 I25 | IATA 2/5 Industrial 2/5 Matrix 2/5 Patch Code PDF417 QR UPC-A UPC-A+EAN-2 UPC-A+EAN-5 UPC-E UPC-E+EAN-2 UPC-E+EAN-5

- The `region` element describes the position of the barcode in the ingested media. If Media Server detects a barcode with a supplement, for example EAN-13+EAN-2, the region includes both parts of the barcode.

- The `parentID` element is empty, unless you configure the analysis engine with `Region=Input` in which case it contains the UUID of the input record. This provides a way to link the result with other records (from another analysis task) that supplied the region to analyze. To generate a single record combining the information, you can use the Combine ESP engine and the example Lua script `parentuuidMatch.lua`.

© Copyright 2022 Micro Focus or one of its affiliates
Version 12.11 | Last updated February 2022

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to swpdl.idoldocsfeedback@microfocus.com.

We appreciate your feedback!

Product: IDOL Media Server 12.11

Topic Title: Barcode Analysis Results