Box Connector 12.12

# RequireGSSAuth

Set `RequireGSSAuth` to `True` to enable GSSAPI authentication mode on the Box Connector service port. In this mode, all connections to the service port must be authenticated using GSSAPI and the Negotiate HTTP authentication mechanism.

To use GSSAPI authentication, you must also set GSSServiceName, to define the GSSAPI service name that Box Connector must use to identify itself.

NOTE: This method provides an authentication requirement only. Micro Focus recommends that you use it in conjunction with TLS/SSL to encrypt the authentication data.

You cannot use `RequireGSSAuth` with GSS ACI encryption (see ACI Encryption Configuration Parameters). If you configure both, Box Connector does not start.

Type: | Boolean
Default: | False
Required: | No
Configuration Section: | Service
Example: | `RequireGSSAuth=True`
See Also: | GSSServiceName

© Copyright 2022 Micro Focus or one of its affiliates
Version 12.12 | Last updated June 2022

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to swpdl.idoldocsfeedback@microfocus.com.

We appreciate your feedback!

Product: IDOL Box Connector 12.12

Topic Title: RequireGSSAuth