Distributed Index Handler 12.13

# DIHEngine`N` Configuration

In the `[DIHEngines]` section you must create a `[DIHEnginwN]` subsection for each child server that the DIH communicates with. Each `[DIHEngineN]` subsection specifies the host and ACI port of a child server, as well as any other optional configuration parameters.

NOTE: You must number child server configuration sections in consecutive order, starting from 0.

For example:

    [DIHEngines]
    Number=2

    [DIHEngine0]
    Host=localhost
    Port=9000

    [DIHEngine1]
    Host=12.3.4.56
    Port=9000

© Copyright 2022 Micro Focus or one of its affiliates
Version 12.13 | Last updated October 2022

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to swpdl.idoldocsfeedback@microfocus.com.

We appreciate your feedback!

Product: IDOL Distributed Index Handler 12.13

Topic Title: DIHEngineN Configuration