Open topic with navigation

# ServicePort

The port on the host server on which the service listens for service status and control requests.

You must configure Authorization Roles Configuration Parameters to determine the users that can send service requests.

Type: | Long
Default: | 40010
Required: | Yes
Allowed Range: | Minimum: 1 Maximum: 65535
Recommended Range: | Minimum: 1024 Maximum: 65535
Configuration Section: | Service
Example: | `ServicePort=40010`
See Also: | ServiceACIMode ServiceHost

© Copyright 2019 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm