Open topic with navigation

# Retrieve Real-Time Data

To create a fetch task to retrieve real-time data from a Gnip stream, follow these steps.

To create a new Fetch Task

1. Stop the connector.
2. Open the configuration file in a text editor.

3. In the `[FetchTasks]` section of the configuration file, specify the number of fetch tasks using the `Number` parameter. If you are configuring the first fetch task, type `Number=1`. If one or more fetch tasks have already been configured, increase the value of the `Number` parameter by one (1). Below the `Number` parameter, specify the names of the fetch tasks, starting from zero (0). For example:

       [FetchTasks]
       Number=1
       0=MyTask

4. Below the `[FetchTasks]` section, create a new TaskName section. The name of the section must match the name of the new fetch task. For example:

       [FetchTasks]
       Number=1
       0=MyTask

       [MyTask]

1. In the new section, set the following configuration parameters:

   `BasicUsername` | The username to use to access Gnip. Micro Focus recommends you encrypt the value of this parameter before adding it to the configuration file. For information about how to encrypt parameter values, see Encrypt Passwords.
   `BasicPassword` | The password to use to access Gnip. Micro Focus recommends you encrypt the value of this parameter before adding it to the configuration file. For information about how to encrypt parameter values, see Encrypt Passwords.
   `StreamUrl` | The URL for the Gnip stream to use. You can find the URLs of your streams at https://console.gnip.com/.

2. If you intend to retrieve entries from a stream that provides a high volume of data, Micro Focus recommends increasing the value of the `IngestBatchSize` parameter. Find the `[Ingestion]` section of the configuration file and set the parameter `IngestBatchSize` to `1000` or more:

       [Ingestion]
       ...
       IngestBatchSize=1500

3. (Optional) If the connector is installed on a machine that is behind a proxy server, you might also need to set some additional configuration parameters so that the connector can access the internet. For more information, see Use a Proxy Server to Access Gnip.

4. Save and close the configuration file.

© Copyright 2019 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a web mail client, and send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm