# DIHEngine`N` Configuration

In the `[DIHEngines]` section you must create a `[DIHEnginwN]` subsection for each child server that the DIH communicates with. Each `[DIHEngineN]` subsection specifies the host and ACI port of a child server, as well as any other optional configuration parameters.

NOTE: You must number child server configuration sections in consecutive order, starting from 0.

For example:

    [DIHEngines]
    Number=2

    [DIHEngine0]
    Host=localhost
    Port=9000

    [DIHEngine1]
    Host=12.3.4.56
    Port=9000

© Copyright 2020 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a mail client, and then send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm