# Identify Vehicle Colors

Media Server can detect the color of vehicles identified by vehicle model recognition.

To detect the color of vehicles

1. Create a new configuration to send to Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Session]` section, add a new analysis task by setting the `EngineN` parameter. You can give the task any name, for example:

       [Session]
       Engine0=Ingest
       Engine1=ANPR
       Engine2=VehicleModel
       Engine3=VehicleColor

3. Create a new section in the configuration file to contain the task settings and set the following parameters:

   `Type` | The analysis engine to use. Set this parameter to `ColorCluster`.
   `Input` | The image track to process. This must be the `ColorRegionWithSource` output track from a vehicle recognition task. This track contains a region that can be used to analyze the vehicle's color. You can customize the selection of this region by setting the parameter `ColorRegion` in your vehicle recognition task, but in most cases the default value provides the greatest accuracy.
   `RestrictToInputRegion` | A Boolean value that specifies whether to analyze a region of the input image or video frame that is specified in the input record, instead of the entire image. Set this parameter to `TRUE`, because you want to analyze only the region that represents the vehicle, and not the entire image.
   `ColorDictionary` | (Optional but recommended) To match vehicle colors against the colors that are defined in a dictionary, specify a dictionary file. Micro Focus recommends that you use the supplied dictionary file `weightedcarcolors.dat`, which is optimized for analyzing color regions derived by the default `ColorRegion` setting in the vehicle recognition task.
   `ColorThreshold` | (Optional) Any color cluster with a score that does not meet the specified threshold is omitted from the results.
   `ColorSpace` | (Optional) The color space in which the results are provided (`RGB`, `YCbCr`, `HSL`, `HSV`, `CIELAB`).

   For example:

       [VehicleColor]
       Type=ColorCluster
       Input=VehicleModel.ColorRegionWithSource
       RestrictToInputRegion=TRUE
       ColorDictionary=weightedcarcolors.dat
       ColorThreshold=20

   For more information about the parameters that customize color analysis, refer to the Media Server Reference.

4. Save and close the configuration file. Micro Focus recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

© Copyright 2020 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a mail client, and then send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm