# Example Barcode Task Configuration

To detect and read barcodes, you could use the following task configuration:

    [Barcodes]
    Type=barcode
    BarcodeTypes=all
    Orientation=any

Setting the `BarcodeTypes` parameter to `all` detects all types of barcodes, including QR codes.

By default Media Server only detects barcodes that are upright, but setting the `Orientation` parameter to `any` means that Media Server can also detect barcodes that have been rotated by 90 or 180 degrees.

© Copyright 2020 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a mail client, and then send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm