# RedRegion0

The position of the red light.

Specify the region using a comma-separated list of values in the order: `left`,`top`,`width`,`height`. These represent:

- The distance between the left of the frame and the left side of the region.
- The distance between the top of the frame and the top of the region.
- The width of the region.
- The height of the region.

Depending on the setting of the RegionUnit parameter, values are given in either pixels or as percentages of the image dimensions. The top-left pixel has the coordinates `0,0`.

Type: | Comma-separated list of integers
Default: |
Required: | Yes
Configuration Section: | TaskName
Example: | `RedRegion0=200,500,20,20 RegionUnit=pixel`
See Also: | RegionUnit

© Copyright 2020 Micro Focus or one of its affiliates | Send documentation feedback Close Send documentation feedback To open the configured email client on this computer, open an email window. Otherwise, copy the information below to a mail client, and then send this email to swpdl.idoldocsfeedback@microfocus.com. We appreciate your feedback! Product: Topic Title: Help Topic: Feedback:

_FT_HTML5_bannerTitle.htm