# MinTimeInterval

DEPRECATED: The `MinTimeInterval` parameter is deprecated in Media Server 12.3.0 and later. Micro Focus recommends that you use the TimestampCondition parameter instead.

This configuration parameter is still available for existing implementations, but it might be incompatible with new functionality. The parameter might be removed in future.

The minimum time from a record in the Input0 track to a record in another track, for the records to be combined. (The engine compares the timestamp values.)

This value can be negative, meaning that the other track's event can occur before the Input0 record.

NOTE: This parameter is used only when you process video. When you process images or documents, this parameter is ignored and records are considered to be related only if they are associated with the same page.

Type: | Time duration The value of this parameter is a time duration. Specify the duration in the following format:
         1days 2hours 3minutes 4seconds 500milliseconds 600microseconds
You can omit any of the individual durations when they are not required:
         4seconds 500milliseconds
You can also shorten the string by abbreviating the units to their first letter (milliseconds abbreviates to ms, microseconds to us):
         4s 500ms
The following are all equivalent:
         1minute 3seconds
         1m 3s
         63s
Default: | Negative of MaxTimeInterval value
Required: | No
Configuration Section: | TaskName
Example: | `MinTimeInterval=-100ms`
See Also: |

_FT_HTML5_bannerTitle.htm