Distributed Action Handler 23.3

# Configure SSL in a Stand-Alone System

Use the following procedure to configure SSL in a setup where you configure the DAH in the stand-alone DAH configuration file.

To configure an SSL connection in a stand-alone system

1. Open the DAH configuration file in a text editor.

2. Find either the `[Server]` section, the `[DistributedEngineN]` section, or both.

3. Add the `SSLConfig` setting to specify the section in which you have set the SSL details for the connection, usually `SSLOptionN`. For example:

       [Server]
       (other server settings...)
       SSLConfig=SSLOption0

       [DistributedEngine0]
       SSLConfig=SSLOption0

       [DistributedEngine1]
       SSLConfig=SSLOption1

   In this example, incoming ACI calls and outgoing calls to `DistributedEngine0` share the same SSL configuration, and outgoing calls to `DistributedEngine1` use a different configuration.

4. Create an `[SSLOptionN]` section for each unique `SSLConfig` setting. Each `SSLOption` entry must contain the `SSLMethod`, `SSLCertificate`, and `SSLPrivateKey` parameters. For example:

       [SSLOption0]
       SSLMethod=TLSV1.3
       SSLCertificate=host1.crt
       SSLPrivateKey=host1.key

       [SSLOption1]
       SSLMethod=TLSV1.3
       SSLCertificate=host2.crt
       SSLPrivateKey=host2.key

5. Save and close the configuration file.

6. Restart the DAH for your changes to take effect.

Copyright 2023 Open Text
Version 23.3 | Last updated June 2023

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to swpdl.idoldocsfeedback@microfocus.com.

We appreciate your feedback!

Product: IDOL Distributed Action Handler 23.3

Topic Title: Configure SSL in a Stand-Alone System