Media Server 23.3

# Write Video to a Rolling Buffer

To write ingested video to a rolling buffer, follow these steps.

To write video to a rolling buffer

1. Create a new configuration to send to Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Session]` section, add a new task by setting the `EngineN` parameter. You can give the task any name, for example:

       [Session]
       Engine0=Ingest
       Engine1=RollingBuffer

3. Create a new configuration section to contain the task settings, and set the following parameters:

   `Type` | The type of engine to use. Set this parameter to `RollingBuffer`.
   `Stream` | The name of the rolling buffer to write video to. You must have created the rolling buffer (see Set Up Rolling Buffers).
   `AudioProfile` | The audio encoding profile to use.
   `VideoProfile` | The video encoding profile to use.

   For example:

       [RollingBuffer]
       Type=RollingBuffer
       Stream=NewsChannel
       AudioProfile=mpeg4audio
       VideoProfile=mpeg4video_h264_sd

4. Save and close the configuration file. OpenText recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

Copyright 2023 Open Text
Version 23.3 | Last updated June 2023

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to swpdl.idoldocsfeedback@microfocus.com.

We appreciate your feedback!

Product: IDOL Media Server 23.3

Topic Title: Write Video to a Rolling Buffer