Distributed Index Handler 24.1

# DIHEngine`N` Configuration

In the `[DIHEngines]` section you must create a `[DIHEnginwN]` subsection for each child server that the DIH communicates with. Each `[DIHEngineN]` subsection specifies the host and ACI port of a child server, as well as any other optional configuration parameters.

NOTE: You must number child server configuration sections in consecutive order, starting from 0.

For example:

    [DIHEngines]
    Number=2

    [DIHEngine0]
    Host=localhost
    Port=9000

    [DIHEngine1]
    Host=12.3.4.56
    Port=9000

Copyright 2023 Open Text
Version 24.1 | Last updated December 2023

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: IDOL Distributed Index Handler 24.1

Topic Title: DIHEngineN Configuration