Vantara Connector 24.3

# Configure Incoming SSL Connections

To configure a connector to accept data sent to its ACI port over SSL, follow these steps.

To configure an incoming SSL Connection

1. Stop the connector.
2. Open the configuration file in a text editor.
3. In the `[Server]` section set the `SSLConfig` parameter to specify the name of a section in the configuration file for the SSL settings. For example:

       [Server]
       SSLConfig=SSLOptions

4. Create a new section in the configuration file (the name must match the name you used in the `SSLConfig` parameter). Then, use the SSL configuration parameters to specify the details for the connection. You must set the following parameters:

   `SSLMethod` | The SSL protocol to use.
   `SSLCertificate` | The SSL certificate to use (in PEM format).
   `SSLPrivateKey` | The private key for the SSL certificate (in PEM format).

   For example:

       [SSLOptions]
       SSLMethod=TLSV1.3
       SSLCertificate=host1.crt
       SSLPrivateKey=host1.key

5. Save and close the configuration file.
6. Restart the connector.

Related Topics

- Start and Stop the Connector

Copyright 2024 Open Text
Version 24.3 | Last updated June 2024

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: IDOL Vantara Connector 24.3

Topic Title: Configure Incoming SSL Connections