AEM Connector 25.1
AEM Connector Help

# PerfMonQueryFrequency

The amount of time, in seconds, that the connector waits between taking readings from a performance counter.

NOTE: Performance monitoring is supported on Windows platforms only.

Type: | Integer
Default: | 5
Recommended Range: | Minimum: 1 Maximum: 10
Required: | No
Configuration Section: | TaskName or FetchTasks
Example: | `PerfMonQueryFrequency=10`
See Also: | PerfMonAvgOverReadings PerfMonCounterMaxN PerfMonCounterMinN PerfMonCounterNameN

Copyright 2024 Open Text
Version 25.1 | Last updated January 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery AEM Connector 25.1

Topic Title: PerfMonQueryFrequency