Media Server 25.1
Media Server Help

# MaxProcessingSessions

The maximum number of processing sessions to start concurrently as a result of requests from upstream Media Servers. If you do not want to accept any requests from upstream Media Servers, set this parameter to `0`.

This parameter limits the number of requests started by upstream servers through Post output tasks, but not through remote analysis. To limit the number of processing sessions that are started as a result of remote analysis requests, use the configuration parameter RemoteAnalysisConfigurations.

If this limit is exceeded the additional requests are queued. Requests can remain in the queue unless they reach the timeout specified by QueueTimeout. When a request is queued, the upstream Media Server does not start ingesting media until the downstream Media Server is ready to begin processing.

TIP: Requests from upstream Media Servers are not started using the `process` action, so this parameter and `[Process]` `MaximumThreads` are not related.

Type: | Integer
Default: | 1
Required: | No
Configuration Section: | Chaining
Example: | `MaxProcessingSessions=3`
See Also: | QueueTimeout

Copyright 2024 Open Text
Version 25.1 | Last updated January 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.1

Topic Title: MaxProcessingSessions