Media Server 25.1
Media Server Help

# RedCyclesPerMinute

The range of acceptable frequencies for flashing red lights.

This parameter is used only for traffic lights at level crossings.

Type: | Custom
Default: | No restriction
Required: | No
Configuration Section: | TaskName
Example: | The following example specifies that the red light can turn on and off (one full cycle) between 8 and 20 times per minute: `RedCyclesPerMinute=8-20`
See Also: |

Copyright 2024 Open Text
Version 25.1 | Last updated January 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.1

Topic Title: RedCyclesPerMinute