Media Server 25.1
Media Server Help

# Detect and Read Number Plates

Media Server can detect and read number plates that appear in video.

To detect and read number plates in video

1. Create a new configuration to send to Media Server with the `process` action, or open an existing configuration that you want to modify.

2. In the `[Session]` section, add a new analysis task by setting the `EngineN` parameter. You can give the task any name, for example:

       [Session]
       Engine0=Ingest
       Engine1=ANPR

3. Create a new section in the configuration file to contain the task settings and set the following parameters:

   `Type` | The analysis engine to use. Set this parameter to `numberplate`.
   `Input` | (Optional) The image track to process. If you do not specify an input track, Media Server processes the first track of the correct type that is produced by the ingest engine.
   Location | (Set this or `LocationWithPriorities`) A comma-separated list of ISO-3166 codes to specify the locations for which you want to recognize number plates. Specify the primary location first. For example, if you are recognizing number plates in France but also want to recognize plates from Germany and Belgium, set this parameter to `Location=FR,DE,BE`.
   LocationWithPriorities | (Set this or `Location`) A comma-separated list of ISO-3166 codes to specify the locations for which you want to recognize number plates, and their relative priorities. For example, if you are recognizing number plates in France but are near the border and also want to recognize plates from Germany and Belgium, you might set `LocationWithPriorities=fr:1.0,de:0.1,be:0.01`. This instructs Media Server that French, German, and Belgian number plates are expected, but German plates are 10 times less likely to be seen than French plates, and Belgian number plates are 100 times less likely to be seen than French plates.
   Region | (Optional) The region of interest (ROI) to monitor for number plates (left, top, width, height, followed by units). If you do not specify a region, Media Server detects and reads number plates anywhere in the scene.
   Sensitivity | (Optional) The confidence level required to detect a number plate.
   MinValidScore | (Optional) The average character score required for a number plate to be recognized.

   For example:

       [ANPR]
       Type=numberplate
       Location=GB
       Region=20,10,60,90 percent
       Sensitivity=14

   For more information about the parameters that customize number plate recognition, see Number Plate Recognition.

4. Save and close the configuration file. OpenText recommends that you save your configuration files in the location specified by the `ConfigDirectory` parameter.

Copyright 2024 Open Text
Version 25.1 | Last updated January 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.1

Topic Title: Detect and Read Number Plates