Media Server 25.1
Media Server Help

# Video Segmentation

Video segmentation divides video into segments that end with a transition to the next scene. Video segmentation is similar to finding keyframes, but can handle more complex transitions.

Configuration Parameter | Description
--- | ---
GradualChangeFrames | The number of frames to consider when looking for gradual scene changes.
Input | The input track.
MinSegmentDuration | The minimum duration of a video segment.
MinStableFrames | The minimum number of successive frames that must be similar for Media Server to consider a transition to be finished.
SampleInterval | The interval at which frames are selected to be analyzed.
Type | The engine to use. Set this parameter to `VideoSegmentation`.

## Output Tracks

The following table describes the tracks that are generated by this engine. The Output column indicates whether the information contained in the track is included by default in the output created by an output task (when you don't set the `Input` parameter for the output task).

Output track | Description | Output
--- | --- | ---
`Data` | Contains one record, describing the analysis results, per video frame. | No
`DataWithSource` | The same as the `Data` track, but each record also includes the source frame. | No
`Result` | Contains one record, describing the analysis results, for each video segment. Each segment includes the transition to the next scene, so every video frame is included in exactly one segment. Each record includes the following fields. `transition` provides the type of transition: `Cut` or `Cut to solid frame` - a sudden change between two adjacent frames. `Transition` or `Transition to solid frame` - successive "cuts" within MinStableFrames of each other, for example a rapid sequence of images. `Fade` or `Fade to solid frame` - a reduction in contrast that happens over multiple frames. where "to solid frame" indicates that the transition ends on a mostly blank frame. `transitionDuration` provides the duration of the transition, so the end of the useful content in a video segment can be determined by taking the end timestamp and subtracting the `transitionDuration`. | Yes
`ResultWithSource` | The same as the `Result` track, but each record also includes the best source frame. | No
`Start` | The same as the `Data` track, except it contains only the first record of each event. | No
`End` | The same as the `Data` track, except it contains only the last record of each event. | No

Copyright 2024 Open Text
Version 25.1 | Last updated January 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.1

Topic Title: Video Segmentation