Media Server 25.1
Media Server Help

# MxPEG Ingest Engine

The MxPEG ingest engine ingests MxPEG video (but not audio) from a file or stream.

NOTE: To ingest MxPEG video from a file you must set the parameter IngestRate to `0`.

Configuration Parameter | Description
--- | ---
StreamTimeout | The maximum amount of time to wait for the next frame.
Type | The type of ingest engine to use. Set this parameter to `MxPEG`.

The MxPEG ingest engine produces the following tracks, where `taskName` is the name of the ingest task:

- `taskName.Image_1` - an image track that contains the video frames. This track can be referred to using the alias `Default_Image`.
- `taskName.Proxy` - the proxy track.

Copyright 2024 Open Text
Version 25.1 | Last updated January 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.1

Topic Title: MxPEG Ingest Engine