Community Component 25.2
Community Component Help

# SleepBetweenRequests

The length of time (in milliseconds) that the Community component mailing operation must wait after it has responded to a request before it can respond to the next request. You can use this option to slow the mailing operation down if it takes too much processing time away from Community.

Type: | Long
Default: | 0
Allowed Range: | Minimum: 0 Maximum: 1638400
Required: | No
Configuration Section: | `MyCustomFunctionality`
Example: | `SleepBetweenRequests=60`
See Also: | RunMailer

Copyright 2025 Open Text
Version 25.2 | Last updated April 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Community Component 25.2

Topic Title: SleepBetweenRequests