Community Component 25.2
Community Component Help

# [DIHEngineN] Section

Use this section when you are using a unified configuration with the Distributed Action Handler and Distributed Index Handler components for a distributed setup. In this case, you configure DAH and DIH in the unified configuration file, and distribute actions to child Content components.

Each `[DIHEngineN]` section define the host and port of a child server that the DIH communicates with.

Use this option to configure the child servers when you want to configure different child servers for the DAH and DIH. For example, you might be using a chained DIH and DAH architecture, such that the top-level DAH distributes actions to child DAH components, and the top-level DIH distributes actions to child DIH components.

You must number child server sections in consecutive order, starting from 0 (zero).

For example:

    [DIHEngines]
    Number=2

    [DIHEngine0]
    Host=dih1.company.com
    Port=16100

    [DIHEngine1]
    Host=12.3.4.56
    Port=16200

Copyright 2025 Open Text
Version 25.2 | Last updated April 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Community Component 25.2

Topic Title: [DIHEngineN] Section