Media Server 25.2
Media Server Help

# RedRegion1

The position of the second red light.

This parameter is used only for traffic lights at level crossings.

Specify the region as a comma-separated list of values in the order: `left,top,width,height`, followed by the units that you want to use.

- `left` is the distance from the left of the frame to the left edge of the region.
- `top` is the distance from the top of the frame to the top edge of the region.
- `width` is the width of the region.
- `height` is the height of the region.

You can choose the following units:

- `percent` or `%` to use percentages of the image or video dimensions (`left` and `width` as percentages of the width, `top` and `height` as percentages of the height).
- `pixels` or `px` to use numbers of pixels.

Type: | Custom
Default: |
Required: | No
Configuration Section: | TaskName
Example: | `RedRegion1=200,500,20,20 pixels`
See Also: |

Copyright 2025 Open Text
Version 25.2 | Last updated April 2025

Send documentation feedback

Close

Send documentation feedback

To send feedback using your default email client, open an email window.

Otherwise, send your feedback and the information below to MFI-swpdl.idoldocsfeedback@opentext.com.

We appreciate your feedback!

Product: Knowledge Discovery Media Server 25.2

Topic Title: RedRegion1